| Index

| Reference for Wiring 1.0 (ALPHA) 0017+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name |  | ### >> (Bitwise bit shift right)
Examples |  |
    unsigned int value=4;                //  4 = 0000 0100
    unsigned int shift=1;

    value = value >> shift;        // 2 = 0000 0010
    value >>= shift;               // 1 = 0000 0001
Description |  | The left expressions value is moved right by the number of bits specified by the right expression.
Syntax |  |
    expression1 >> expression2
    expression1 >>= expression2
Parameters |  |
expression1 |  | any valid expression
expression2 |  | any valid expression
Returns |  |
Usage |  | Application
Related |  | & (bitwise AND) &= (bitwise AND and assign) | (bitwise OR) |= (bitwise OR and assign) ^ (bitwise XOR) ˜ (bitwise ones complement) << (bitwise bit shift left)