| Index

| Reference for Wiring 1.0 (ALPHA) 0017+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name |  | ### |= (Bitwise OR and assign)
Examples |  |
    unsigned int a = 60;	// 60 = 0011 1100
    unsigned int b = 13;	// 13 = 0000 1101

    a |= b;                 // 61 = 0011 1101
Description |  | Combines bitwise OR and assign. The expression a |= b is equivalent to a = a | b.
Syntax |  |
    expression1 |= expression2
Parameters |  |
expression1 |  | any valid expression
expression2 |  | any valid expression
Returns |  |
Usage |  | Application
Related |  | & (bitwise AND) &= (bitwise AND and assign) | (bitwise OR) ^ (bitwise XOR) ˜ (bitwise ones complement) << (bitwise bit shift left) >> (bitwise bit shift right)